MESH2D
NUM_MATERIALS_PER_ELEM 1 
BEGPARAMDEF
GM  "RiverFLO-2D"
SI  0
DY  0
TU  "Hours"
TD  0  0
GP 1 "Control Data" 1
GP_DEF  1 1 "Simulation Time (hrs)" 2 0 0 1.79769e+308
GP_DEF  1 2 "Output Interval (hrs)" 2 0 0 1.79769e+308
GP_DEF  1 3 "Timestep (sec)" 2 0 0 1.79769e+308
GP_DEP 1 3 "PARENT_SELF" "Variable Timestep" 0 "On" 0 "Off" 1 
GP_DEF  1 4 "Variable Timestep" 4 "On"
GP_OPTS 1 4  "On" "Off"
GP_DEF  1 5 "     Variable Timestep Multiplier" 2 1 0 1.79769e+308
GP_DEP 1 5 "PARENT_SELF" "Variable Timestep" 1 "On" 1 "Off" 0 
GP_DEF  1 6 "Simulation Type" 4 "Steady State"
GP_OPTS 1 6  "Steady State" "Transient"
GP_DEF  1 7 "Initial Conditions" 4 "Dry Bed"
GP_OPTS 1 7  "Dry Bed" "Horizontal Water Surface" "Define Initial WSE as Dataset"
GP_DEF  1 8 "     Horizontal Water Surface Elevation" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 1 8 "PARENT_SELF" "Initial Conditions" 0 "Dry Bed" 0 "Horizontal Water Surface" 1 "Define Initial WSE as Dataset" 0 
GP_DEF  1 9 "     XMDF File Name" 3 "Datasets.h5"
GP_DEP 1 9 "PARENT_SELF" "Initial Conditions" 0 "Dry Bed" 0 "Horizontal Water Surface" 0 "Define Initial WSE as Dataset" 1 
GP_DEF  1 10 "     Mesh Dataset Name" 3 "Initial WSE"
GP_DEP 1 10 "PARENT_SELF" "Initial Conditions" 0 "Dry Bed" 0 "Horizontal Water Surface" 0 "Define Initial WSE as Dataset" 1 
GP_DEF  1 11 "Wetting/Drying Method" 4 "A"
GP_OPTS 1 11  "A" "B"
GP_DEF  1 12 "Minimum Depth for Dry Bed" 2 0.1 0 1.79769e+308
GP_DEF  1 13 "Use Hotstart Run" 4 "On"
GP_OPTS 1 13  "On" "Off"
GP_DEF  1 14 "     Hotstart file name (.VTPA)" 3 "TIME_ENG_0000_00_00_00.EXP"
GP_DEP 1 14 "PARENT_SELF" "Use Hotstart Run" 0 "On" 1 "Off" 0 
GP_DEF  1 15 "Text File Output" 0 0
GP_DEP 1 15 "PARENT_SELF" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
GP_DEF  1 16 "Slip Boundary Condition" 4 "Slip"
GP_OPTS 1 16  "Slip" "Non-Slip" "Semi-Slip"
GP_DEP 1 16 "PARENT_SELF" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
GP_DEF  1 17 "     Semi-Slip Multiplier" 2 1 0 1
GP_DEP 1 17 "PARENT_SELF" "Slip Boundary Condition" 0 "Slip" 0 "Non-Slip" 0 "Semi-Slip" 1 
GP_DEF  1 18 "Selective Lumping Parameter" 2 0.9 0.8 0.99
GP_DEP 1 18 "PARENT_SELF" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
GP_DEF  1 19 "Manning's N Multiplier" 2 1 0.1 2
GP_DEP 1 19 "PARENT_SELF" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
GP_DEF  1 20 "Cross Sections Output File" 0 0
GP_DEP 1 20 "PARENT_SELF" "Variable Timestep" 1 "On" 1 "Off" 1 
GP_DEF  1 21 "Profile Output File" 0 0
GP_DEP 1 21 "PARENT_SELF" "Variable Timestep" 1 "On" 1 "Off" 1 
GP 2 "Sediment Transport" 1
GP_DEF  2 1 "Sediment Transport" 4 "Off"
GP_OPTS 2 1  "Off" "On"
GP_DEF  2 2 "Transport Formula" 4 "Rating Formula"
GP_OPTS 2 2  "Rating Formula" "Meyer-Peter & Muller" "Karim-Kennedy" "Ackers-White" "Yang (Sand)" "Yang (Gravel)" "Parker-Klingeman-Mclean" "Van Rijn" "Engelund Hansen"
GP_DEP 2 2 "PARENT_SELF" "Sediment Transport" 0 "Off" 0 "On" 1 
GP_DEF  2 3 "Sediment Transport Timestep Ratio" 1 1 0 2147483647
GP_DEP 2 3 "PARENT_SELF" "Transport Formula" 0 "Rating Formula" 1 "Meyer-Peter & Muller" 1 "Karim-Kennedy" 1 "Ackers-White" 1 "Yang (Sand)" 1 "Yang (Gravel)" 1 "Parker-Klingeman-Mclean" 1 "Van Rijn" 1 "Engelund Hansen" 1 
GP_DEF  2 4 "Erosion Depth Options" 4 "Constant"
GP_OPTS 2 4  "Constant" "Defined as Dataset"
GP_DEP 2 4 "PARENT_SELF" "Sediment Transport" 0 "Off" 0 "On" 1 
GP_DEF  2 5 "     Max Erosion Depth" 2 0 0 1.79769e+308
GP_DEP 2 5 "PARENT_SELF" "Erosion Depth Options" 0 "Constant" 1 "Defined as Dataset" 0 
GP_DEF  2 6 "     XMDF File Name" 3 "Datasets.h5"
GP_DEP 2 6 "PARENT_SELF" "Erosion Depth Options" 0 "Constant" 0 "Defined as Dataset" 1 
GP_DEF  2 7 "     Mesh Dataset" 3 "MaxDepth"
GP_DEP 2 7 "PARENT_SELF" "Erosion Depth Options" 0 "Constant" 0 "Defined as Dataset" 1 
GP_DEF  2 8 "D50 (mm)" 2 0 0 1.79769e+308
GP_DEP 2 8 "PARENT_SELF" "Transport Formula" 0 "Rating Formula" 1 "Meyer-Peter & Muller" 1 "Karim-Kennedy" 1 "Ackers-White" 1 "Yang (Sand)" 1 "Yang (Gravel)" 1 "Parker-Klingeman-Mclean" 1 "Van Rijn" 1 "Engelund Hansen" 1 
GP_DEF  2 9 "D90 (mm)" 2 0 0 1.79769e+308
GP_DEP 2 9 "PARENT_SELF" "Transport Formula" 0 "Rating Formula" 0 "Meyer-Peter & Muller" 0 "Karim-Kennedy" 0 "Ackers-White" 0 "Yang (Sand)" 0 "Yang (Gravel)" 0 "Parker-Klingeman-Mclean" 0 "Van Rijn" 1 "Engelund Hansen" 0 
GP_DEF  2 10 "Sediment Specific Gravity" 2 2.65 2 2.7
GP_DEP 2 10 "PARENT_SELF" "Transport Formula" 0 "Rating Formula" 1 "Meyer-Peter & Muller" 1 "Karim-Kennedy" 1 "Ackers-White" 1 "Yang (Sand)" 1 "Yang (Gravel)" 1 "Parker-Klingeman-Mclean" 1 "Van Rijn" 1 "Engelund Hansen" 1 
GP_DEF  2 11 "Bed Sediment Porosity" 2 0.4 0.3 0.6
GP_DEP 2 11 "PARENT_SELF" "Transport Formula" 0 "Rating Formula" 0 "Meyer-Peter & Muller" 1 "Karim-Kennedy" 1 "Ackers-White" 1 "Yang (Sand)" 1 "Yang (Gravel)" 1 "Parker-Klingeman-Mclean" 1 "Van Rijn" 1 "Engelund Hansen" 1 
GP_DEF  2 12 "A" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 2 12 "PARENT_SELF" "Transport Formula" 0 "Rating Formula" 1 "Meyer-Peter & Muller" 0 "Karim-Kennedy" 0 "Ackers-White" 0 "Yang (Sand)" 0 "Yang (Gravel)" 0 "Parker-Klingeman-Mclean" 0 "Van Rijn" 0 "Engelund Hansen" 0 
GP_DEF  2 13 "B" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 2 13 "PARENT_SELF" "Transport Formula" 0 "Rating Formula" 1 "Meyer-Peter & Muller" 0 "Karim-Kennedy" 0 "Ackers-White" 0 "Yang (Sand)" 0 "Yang (Gravel)" 0 "Parker-Klingeman-Mclean" 0 "Van Rijn" 0 "Engelund Hansen" 0 
GP 3 "Rainfall/Evaporation" 0
GP_DEF  3 1 "Rainfall/Evaporation" 4 "Off"
GP_OPTS 3 1  "Off" "On"
GP_DEF  3 2 "Rainfall" 5 "Time (hrs)" "Rainfall (mm)" 
GP_DEP 3 2 "PARENT_SELF" "Rainfall/Evaporation" 0 "Off" 0 "On" 1 
GP_DEF  3 3 "Evaporation" 5 "Time (hrs)" "Evaporation (mm)" 
GP_DEP 3 3 "PARENT_SELF" "Rainfall/Evaporation" 0 "Off" 0 "On" 1 
GP 4 "Graphic Output Options" 0
GP_DEF  4 1 "Graphic Output Options" 4 "Default"
GP_OPTS 4 1  "Default" "Specify Options"
GP_DEF  4 2 "Plot Type" 4 "Velocity Field (Black)"
GP_OPTS 4 2  "Velocity Field (Black)" "Velocity Fields (Color)" "Velocities & Depth" "Velocities & Bed Elevations" "Depths" "Bed Elevations"
GP_DEP 4 2 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 3 "Color Scheme" 4 "1"
GP_OPTS 4 3  "1" "2" "3" "4" "5"
GP_DEP 4 3 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 4 "Plot Axis" 0 0
GP_DEP 4 4 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 5 "Create DXF " 0 0
GP_DEP 4 5 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 6 "Create Graphic Output Files " 0 0
GP_DEP 4 6 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 7 "Velocity Vector Factor" 2 2 0 1.79769e+308
GP_DEP 4 7 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 8 "Max Velocity Vector" 2 2 0 1.79769e+308
GP_DEP 4 8 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 9 "Min Variable Limit" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 4 9 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 10 "Max Variable Limit" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 4 10 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 11 "Plot Window X1" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 4 11 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 12 "Plot Window Y1" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 4 12 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 13 "Plot Window X2" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 4 13 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP_DEF  4 14 "Plot Window Y2" 2 0 -1.79769e+308 1.79769e+308
GP_DEP 4 14 "PARENT_SELF" "Graphic Output Options" 1 "Default" 0 "Specify Options" 1 
GP 5 "Component Controls" 0
GP_DEF  5 1 "Piers" 0 0
GP_DEF  5 2 "Weirs" 0 0
GP_DEF  5 3 "Culverts" 0 0
GP_DEF  5 4 "Sources/Sinks" 0 0
GP_DEF  5 5 "Internal Rating Curve" 0 0
NUME  3
BCPGC  1
DISP_OPTS entity   0 0 0 0 1 0 0 0
DISP_OPTS inactive 0 0 0 0 1 0 0 0
DISP_OPTS multiple 0 0 0 0 1 0 0 0
BEFONT  0 1
DISP_OPTS entity   1 153 51 51 0 0 0 0
DISP_OPTS inactive 1 153 51 51 1 0 0 0
DISP_OPTS multiple 1 0 0 0 1 0 1 0
BEFONT  1 1
BC  1 "Exterior Boundary Condition" 1 0 1 -1 "Control Data"
BC_DEF 1 1 "Steady State BC Type" 4 "Discharge"
BC_OPTS 1 1  "Discharge" "Water Surface Elevation (WSE)" "Discharge & WSE" "U Velocity" "V Velocity" "U & V Velocity" "WSE & U Velocity" "WSE & V Velocity" "Free Inflow/Outflow" "Free Outflow" "Water & Sediment Discharge" "Discharge as a Source" "Uniform Flow Outflow"
BC_DEP 1 1 "PARENT_GLOBAL" "Simulation Type" 1 "Steady State" 1 "Transient" 0 
BC_DEF 1 2 "Discharge" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 2 "PARENT_LOCAL" "Steady State BC Type" 0 "Discharge" 1 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 1 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 0 "WSE & V Velocity" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 1 "Discharge as a Source" 1 "Uniform Flow Outflow" 0 
BC_DEF 1 3 "Water Surface Elevation" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 3 "PARENT_LOCAL" "Steady State BC Type" 1 "Discharge" 0 "Water Surface Elevation (WSE)" 1 "Discharge & WSE" 1 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 1 "WSE & V Velocity" 1 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 4 "U Velocity" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 4 "PARENT_LOCAL" "Steady State BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 1 "V Velocity" 0 "U & V Velocity" 1 "WSE & U Velocity" 1 "WSE & V Velocity" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 5 "V Velocity" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 5 "PARENT_LOCAL" "Steady State BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 0 "V Velocity" 1 "U & V Velocity" 1 "WSE & U Velocity" 0 "WSE & V Velocity" 1 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 6 "Sediment Discharge" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 6 "PARENT_LOCAL" "Steady State BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 0 "WSE & V Velocity" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 1 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 7 "Transient BC Type" 4 "Discharge"
BC_OPTS 1 7  "Discharge" "Water Surface Elevation (WSE)" "Discharge & WSE" "U Velocity" "V Velocity" "U & V Velocity" "WSE & U Velocity" "WSE & V Velocity" "External Boundary Rating Table" "Free Inflow/Outflow" "Free Outflow" "Water & Sediment Discharge" "Discharge as a Source" "Uniform Flow Outflow"
BC_DEP 1 7 "PARENT_GLOBAL" "Simulation Type" 0 "Steady State" 0 "Transient" 1 
BC_DEF 1 10 "Discharge (Time Series)" 5 "Time" "Discharge" 
BC_DEP 1 10 "PARENT_LOCAL" "Transient BC Type" 0 "Discharge" 1 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 1 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 0 "WSE & V Velocity" 0 "External Boundary Rating Table" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 1 "Discharge as a Source" 1 "Uniform Flow Outflow" 0 
BC_DEF 1 11 "Water Surface Elevation (Time Series)" 5 "Time" "Water Surface Elevation" 
BC_DEP 1 11 "PARENT_LOCAL" "Transient BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 1 "Discharge & WSE" 1 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 1 "WSE & V Velocity" 1 "External Boundary Rating Table" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 12 "U Velocity (Time Series)" 5 "Time" "U Velocity" 
BC_DEP 1 12 "PARENT_LOCAL" "Transient BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 1 "V Velocity" 0 "U & V Velocity" 1 "WSE & U Velocity" 1 "WSE & V Velocity" 0 "External Boundary Rating Table" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 13 "V Velocity (Time Series)" 5 "Time" "V Velocity" 
BC_DEP 1 13 "PARENT_LOCAL" "Transient BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 0 "V Velocity" 1 "U & V Velocity" 1 "WSE & U Velocity" 0 "WSE & V Velocity" 1 "External Boundary Rating Table" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 14 "External Boundary Rating Table" 5 "Discharge" "Water Surface Elevation" 
BC_DEP 1 14 "PARENT_LOCAL" "Transient BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 0 "WSE & V Velocity" 0 "External Boundary Rating Table" 1 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 15 "Sediment Discharge (Time Series)" 5 "Time" "Sediment Discharge" 
BC_DEP 1 15 "PARENT_LOCAL" "Transient BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 0 "WSE & V Velocity" 0 "External Boundary Rating Table" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 1 "Discharge as a Source" 0 "Uniform Flow Outflow" 0 
BC_DEF 1 16 "Energy Slope So" 4 "Calculate So using topography"
BC_OPTS 1 16  "Calculate So using topography" "Provide So"
BC_DEP 1 16 "PARENT_LOCAL" "Steady State BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 0 "WSE & V Velocity" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 1 
BC_DEF 1 17 " Energy Slope So" 4 "Calculate So using topography"
BC_OPTS 1 17  "Calculate So using topography" "Provide So"
BC_DEP 1 17 "PARENT_LOCAL" "Transient BC Type" 0 "Discharge" 0 "Water Surface Elevation (WSE)" 0 "Discharge & WSE" 0 "U Velocity" 0 "V Velocity" 0 "U & V Velocity" 0 "WSE & U Velocity" 0 "WSE & V Velocity" 0 "External Boundary Rating Table" 0 "Free Inflow/Outflow" 0 "Free Outflow" 0 "Water & Sediment Discharge" 0 "Discharge as a Source" 0 "Uniform Flow Outflow" 1 
BC_DEF 1 18 "So" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 18 "PARENT_LOCAL" "Energy Slope So" 0 "Calculate So using topography" 0 "Provide So" 1 
BC_DEF 1 19 " So" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 1 19 "PARENT_LOCAL" " Energy Slope So" 0 "Calculate So using topography" 0 "Provide So" 1 
BC_DISP_OPTS 1 1 0 0 0 1 0 1 1
BC  1 "Interior Boundary Condition" 2 0 1 -1 "Control Data"
BC_DEF 2 1 "Stage Discharge Rating Table" 5 "Discharge" "Water Surface Elevation" 
BC_DEP 2 1 "PARENT_GLOBAL" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
BC_DISP_OPTS 2 1 0 0 0 1 0 1 1
BC  1 "Weir" 3 0 1 -1 "Control Data"
BC_DEF 3 1 "Name" 3 ""
BC_DEP 3 1 "PARENT_GLOBAL" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
BC_DEF 3 2 "Weir Coefficient" 2 0 0 1.79769e+308
BC_DEP 3 2 "PARENT_GLOBAL" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
BC_DISP_OPTS 3 1 0 0 0 1 0 1 1
DISP_OPTS entity   2 0 0 0 1 0 1 1
DISP_OPTS inactive 2 0 0 0 1 0 1 0
DISP_OPTS multiple 2 0 0 0 1 0 1 0
BEFONT  2 1
BC  2 "Pier" 1 0 1 -1 "Control Data"
BC_DEF 1 1 "Pier Name" 3 ""
BC_DEF 1 2 "Angle" 2 0 0 180
BC_DEF 1 3 "Length" 2 0 0 1.79769e+308
BC_DEF 1 4 "Width" 2 0 0 1.79769e+308
BC_DEF 1 5 "Drag Coefficient" 2 0.5 0.5 2.5
BC_DISP_OPTS 1 2 0 0 0 0 0 0 0
BC  2 "Source/Sink" 2 0 1 -1 "Control Data"
BC_DEF 2 1 "Source/Sink ID" 3 ""
BC_DEP 2 1 "PARENT_GLOBAL" "Simulation Type" 1 "Steady State" 1 "Transient" 1 
BC_DEF 2 2 "Discharge" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 2 2 "PARENT_GLOBAL" "Simulation Type" 1 "Steady State" 1 "Transient" 0 
BC_DEF 2 3 "Time Series" 5 "Time (hrs)" "Discharge" 
BC_DEP 2 3 "PARENT_GLOBAL" "Simulation Type" 0 "Steady State" 0 "Transient" 1 
BC_DISP_OPTS 2 2 0 0 0 0 0 0 0
BC  2 "Culvert Inlet" 3 0 1 -1 "Control Data"
BC_DEF 3 1 "Culvert Inlet Name" 3 ""
BC_DEP 3 1 "PARENT_LOCAL" "Culvert Data Options" 1 "Type 0 - Rating Table" 1 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 2 "Culvert Data Options" 4 "Type 0 - Rating Table"
BC_OPTS 3 2  "Type 0 - Rating Table" "Type 1 - Culvert Equations (Box)" "Type 2 - Culvert Equations (Circular)"
BC_DEP 3 2 "PARENT_GLOBAL" "Variable Timestep" 1 "On" 1 "Off" 1 
BC_DEF 3 3 "Culvert Rating Table" 5 "Discharge" "Water Surface Elevation" 
BC_DEP 3 3 "PARENT_LOCAL" "Culvert Data Options" 1 "Type 0 - Rating Table" 1 "Type 1 - Culvert Equations (Box)" 0 "Type 2 - Culvert Equations (Circular)" 0 
BC_DEF 3 4 "Entrance Loss Coefficient (Ke)" 2 0.5 0 1
BC_DEP 3 4 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 5 "Culvert Manning N Coefficient" 2 0 0 1.79769e+308
BC_DEP 3 5 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 6 "Inlet Control Coefficient (Kp)" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 6 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 7 "Inlet Control Coefficient (M)" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 7 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 8 "Inlet Control Coefficient (Cp)" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 8 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 9 "Inlet Control Coefficient (Y)" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 9 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 10 "Inlet Form Coefficient (m)" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 10 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 11 "Number of Identical Barrels (Nb)" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 11 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 1 
BC_DEF 3 12 "Barrel Height" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 12 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 0 
BC_DEF 3 13 "Barrel Width" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 13 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 1 "Type 2 - Culvert Equations (Circular)" 0 
BC_DEF 3 14 "Diameter" 2 0 -1.79769e+308 1.79769e+308
BC_DEP 3 14 "PARENT_LOCAL" "Culvert Data Options" 0 "Type 0 - Rating Table" 0 "Type 1 - Culvert Equations (Box)" 0 "Type 2 - Culvert Equations (Circular)" 1 
BC_DISP_OPTS 3 2 0 0 0 0 0 0 0
BC  2 "Culvert Outlet" 4 0 1 -1 "Control Data"
BC_DEF 4 1 "Culvert Inlet Name" 3 ""
BC_DISP_OPTS 4 2 0 0 0 0 0 0 0
MAT 1 "material 01"
MAT 2 "material 02"
MAT_MULTI 0
MAT_DEF 1 1 "Mannings N" 2 0.035 0 1.79769e+308
ENDPARAMDEF
BEG2DMBC
END2DMBC
BEGCURVE Version: 1
ENDCURVE
